**EFA-TLG® Door Light Grid**

**Door Light Grid**

Self-monitoring, TÜV-tested DOOR LIGHT GRID (EFA-TLG®), fully protected and integrated in the side frames of the door. The light grid acts directly on the door closing level and creates an almost full-surface infrared light curtain up to a height of 2.5 m. Obstacles are detected without contact. The closing movement then stops immediately. This means that reverse operation can be initiated at a much earlier point in time.

Safety edge and/or light barrier(s) are omitted.

Application variant depending on the door type

**Optional:**

Combination of EFA-TLG® and safety edge