**High speed spiral Door, Type „EFA-SST® Alux Eco“**

Manufacturing, delivery, and installation of:

**EFAFLEX** offers the high-speed spiral door type **“EFA-SST® Alux Eco”** for demanding industrial continuous operation. This door combines first-class performance with outstanding durability.

The **door system** consists of galvanized, self-supporting steel frames with a spiral door leaf reception. A dual-sided synchronous shaft ensures even force distribution. Precision ball-bearing rollers provide exact, smooth and quiet guidance of the hinge bands. A spring mechanism certified according to DIN EN 12064 balances the weight of the door leaf, allowing manual opening in case of a power failure.

The **door leaf** is made of double-walled, anodized aluminium laths, fastened in hinge bands and moved vertically. The surface features a two-layer coating in white aluminium (similar to RAL 9006).

The innovative **spiral body** of the door is designed so that the laths of the door leaf pass each other completely contact-free. This guarantees wear-free and quiet operation.

The **door drive** is powered by a high-performance high-frequency geared brake motor. Inductive proximity switches continuously and precisely detect the door positions, with the end positions determined electronically. Electromechanical limit switches are not permitted.

**Opening speed: up to approx. 1,3 m/sec.**

**Maximum door leaf speed: up to approx. 1,5 m/sec.**

(depending on door size)

**Closing speed: up to approx. 1,0 m/sec.**

**The EFA-TRONIC®** control system with integrated frequency converter is housed in a plastic control cabinet (protection class IP 65). Connection to the power supply is made with 230V or 400V at 50 Hz (provided by the customer).

The integrated TÜV-approved door line light grid (**EFA-TLG®**) ensures maximum safety. It is integrated into the side frames and creates a dense infrared light grid up to a height of 2,5 m. Obstacles are detected without contact, and the automatic closing movement is immediately stopped.

Regulations according to DIN EN 13241-1 are fulfilled;

Resistance to wind load according to DIN EN 12424 up to class 5 (+1050 Pa / -1050 Pa)

Air permeability according to DIN EN 12426 class 2

Airborne sound insulation according to DIN EN ISO 7171 up to 25 dB(A)

Thermal insulation according to DIN EN 12428 up to 5,7 W/m²K

(Values depend on door size and equipment)

for clear height:

Width = ............... mm x Height = ............... mm

**Manufacturer‘s certificate:**

EFAFLEX Tor- und Sicherheitssysteme GmbH & Co. KG

[www.efaflex.com](http://www.efaflex.com)

05/2024 Technical changes reserved