**HIGH-SPEED TURBO ROLL-UP DOOR, type “EFA-STR®-L N”**  
Manufacture, delivery and installation of:  
  
high-speed roll-up door, type “EFA-STR®-L N”, with electro-mechanical high-performance door drive for permanent industrial applications  
  
The door system primarily consists of:  
self-supporting steel side frames, steel parts (which are generally galvanised) and spiral-shaped door leaf mounts  
The force is applied on both sides: To achieve this, a synchronised drive is installed. Ball-bearing precision rolling units have to be used for the precise, smooth and low-noise guidance of the hinge chains. A sufficiently dimensioned tension spring mechanism, ensuring the weight balancing of the door leaf and manual opening of the door (e.g. in the case of a power failure), is installed in the door frames, in accordance with DIN EN 12604.   
  
The flexible DOOR LEAF is generally made of wear-free, single-walled PVC fibre and is moved upwards and/or downwards in a force-closed manner. Four standardised segment fields are connected to form individual modules each, which can be exchanged easily and quickly. Curtain colours available: blue, red, yellow and grey. Upon request, a transparent window with a nominal height of about 900 mm is available without surcharge. The curtain is exactly led laterally so that linear expansion is ruled out. Anodised aluminium posts reinforce the door leaf. The modular structure ensures a quick and low-cost exchange of individual sections.  
  
This SPIRAL BODY is designed to guide the laths of the door leaf completely without contact and thus without wear and with best possible noise reduction.   
Spiral form: Low-Header  
The DOOR is driven by a gear brake motor, which must be designed as high-frequency motor. The door positions are detected by means of non-wearing, inductive proximity switches, whereby the limits are determined electronically. Electro-mechanical limit switches are not permissible here.  
  
**OPENING SPEED: up to approx. 2.5 m/s  
Max. DOOR LEAF SPEED: up to approx. 2.8 m/s  
(depending on the door size)  
CLOSING SPEED: up to approx. 1.0 m/s**  
The **MICROPROCESSOR CONTROL** is installed along with the integrated frequency converter in a separate plastic switch cabinet, protection class IP 65. Connection to 230V / 50 Hz power supply on-site.  
  
The scope of delivery includes an electric safety contact edge which is self-monitoring in accordance with DIN EN 12453: The connection cable must be guided and protected within the door frame by an energy chain.  
  
Regulations pursuant to DIN EN 13241-1 are complied with;  
Resistance to wind load in accordance with DIN EN 12424, up to class 3  
Airborne sound insulation in accordance with DIN EN 7171, up to 12 dB(A)  
 (values dependant on the door size and equipment)  
  
  
for clear passage opening dimensions  
Width = ............... mm x Height = ............... mm

**OPTIONS available for the high-speed turbo roll-up door “EFA-STR®-S N”:**  
Surface  
Powder coating of all galvanised steel parts in a colour according to RAL \_\_\_\_\_\_\_\_\_\_ (metallic colours are not available)  
  
Stainless steel version (V2A) of all visible steel parts, visible surface polished, grain size 220,  
incl. switch cabinet made of V2A, incl. guide rollers with V2A bearings, e.g. for wet operations  
  
**Standard speed:**  
Reduced price for version with standard speed:  
OPENING SPEED: up to approx. 1.6 m/s  
Max. DOOR LEAF SPEED: up to approx. 2.0 m/s  
(depending on the lifting height)  
CLOSING SPEED: up to approx. 1.0 m/s  
  
**Alternative safety system:**  
Surcharge for a self-monitoring, TÜV-certified DOOR LINE – LIGHT-LINE CURTAIN (EFA-TLG®), completely safely integrated into the side frame of the door. The light-line curtain is directly active at the door closing level and generates an infrared light curtain which covers almost the entire surface, up to a height of 2.5 metres. Obstacles are detected without contact. This immediately stops the closing movement of the door. Thus, enabling the reversing opening to be initiated at a significantly earlier point in time. Contact edges and/or light barrier(s) are not necessary.