**HIGH-SPEED ROLLER DOOR, Type „EFA-SRT® EasyFit“**

Space-saving high-speed roller door for universal indoor use. Particularly suitable for heavy-duty industrial or commercial use. This door type has been designed for particularly quick installation. At the same time, its clever modular construction means that it is largely maintenance-free, offers a slim design with foldable frames and an attractive price-performance ratio.

**TechniCAL FEATURES**

* Very quick and easy installation thanks to foldable, pre-wired frames.
* Very slim design, manual opening via hand crank possible.
* Door curtain: 0.8 mm polyester fabric (9 colours); optional transparent PVC curtain with warning stripes or Transilon curtain (2 mm, with/without viewing window).
* Surface: Choice of galvanised, stainless steel or powder coating according to RAL.
* EFA-TRONIC® control unit with externally mounted polycarbonate control cabinet and integrated frequency converter.
* Pre-assembled door light grid (TLG) integrated as standard.
* Opening speed up to 1.5 m/s; closing speed up to 1.0 m/s.
* Long service life with up to 150,000 load cycles per year
* Service life of 20 years, including 10 years of product liability law
* Certification: Tested and certified by ift Rosenheim.

**PERFORMANCE VALUES (depending on equipment)**

* Resistance to wind load: DIN EN 12424, Class 2, measured by EFAFLEX, 41 km/h / 87 Pa
* Watertightness: DIN EN 12425, npd
* Air permeability: DIN EN 12426, npd
* Sound insulation: DIN EN ISO 717-1, bis Rw = 11 dB
* Thermal insulation: DIN EN 12428, npd

**dimensions of the clear opening**

Width = ............... mm

Height = ............... mm